Pipe Module Technical Report    Code : VARVE1         

Flow Rate               4.00 l/sec
Suction height          0.00 m
Discharge height        5.11 m
Discharge pressure      0.00 m

Pipe Section           Internal pipe Rising main
Pipes in Parallel                  1           1
Pipe Length                    1.9 m     340.0 m
Nominal Diameter             50.0 mm     90.0 mm
Inside Diameter              52.5 mm     79.2 mm
Pipe Material               ST/STEEL        HDPE
Pipe Roughness             0.5000 mm   0.2500 mm
Pipe Fittings                      5           0
                  1 BALL CHECK VALVE            
                       1 BRANCH PIPE            
                  1 GATE VALVE, open            
                   1 LONG ELBOW, 90ø            
                        1 PUMP STAND            
Reynold's No                   97009       64305
Velocity                    1.85 m/s    0.81 m/s
Friction Loss                                   
  Fittings                     1.2 m       0.0 m
  Pipe                         0.2 m       4.1 m
  Total                        1.4 m       4.1 m

NPSHa              10.01 m
Static head         5.11 m
Friction head       5.50 m
Total head         10.61 m
